<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.5.2">
<drawing>
<board>
<plain>
<wire x1="0.635" y1="-1.905" x2="54.28" y2="-1.905" width="0" layer="20"/>
<wire x1="54.28" y1="71.745" x2="0.635" y2="71.745" width="0" layer="20"/>
<wire x1="0.635" y1="71.745" x2="0.635" y2="-1.905" width="0" layer="20"/>
<wire x1="54.28" y1="-1.905" x2="54.28" y2="71.745" width="0" layer="20"/>
<text>PTN78020 - Robotech V0
5V
10V</text>
<text>VCC
VOUT 1
EN 1
EN2
GND
VOUT2</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="0805-THM">
</package>
</packages>
</library>
<library name="ptn78060wah">
<description>This librarly contains TI's PTN78060 adn PTN78020 3A/6A wide-input adjustable switching
regulator. Only the through-hole versions of the footprints exist. All three footprints are verified.</description>
<packages>
<package name="PTN78020WAH">
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DRIL-3">
<description>&lt;b&gt;MARKER&lt;/b&gt; &lt;p&gt;
drill 3.0 mm'</description>
</package>
</packages>
</library>
<library name="1x2mta">
<description>&lt;b&gt;AMP Connectors&lt;/b&gt;&lt;p&gt;
RJ45 Jack connectors&lt;br&gt;
 Based on the previous libraris:
 &lt;ul&gt;
 &lt;li&gt;amp.lbr
 &lt;li&gt;amp-j.lbr
 &lt;li&gt;amp-mta.lbr
 &lt;li&gt;amp-nlok.lbr
 &lt;li&gt;amp-sim.lbr
 &lt;li&gt;amp-micro-match.lbr
 &lt;/ul&gt;
 Sources :
 &lt;ul&gt;
 &lt;li&gt;Catalog 82066 Revised 11-95 
 &lt;li&gt;Product Guide 296785 Rev. 8-99
 &lt;li&gt;Product Guide CD-ROM 1999
 &lt;li&gt;www.amp.com
 &lt;/ul&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MYJUMPER">
<description>&lt;b&gt;JUMPER REVISITE PAR AMAURY&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="adafruit" package="0805-THM" value=""/>
<element name="R3" library="adafruit" package="0805-THM" value=""/>
<element name="U$1" library="ptn78060wah" package="PTN78020WAH" value="PTN78020WAH"/>
<element name="U$2" library="ptn78060wah" package="PTN78020WAH" value="PTN78020WAH"/>
<element name="U$3" library="special" package="DRIL-3" value=""/>
<element name="U$4" library="special" package="DRIL-3" value=""/>
<element name="U$5" library="special" package="DRIL-3" value=""/>
<element name="U$6" library="special" package="DRIL-3" value=""/>
<element name="J1" library="1x2mta" package="MYJUMPER" value=""/>
<element name="J2" library="1x2mta" package="MYJUMPER" value=""/>
<element name="J3" library="1x2mta" package="MYJUMPER" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$2" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="1"/>
<contactref element="U$2" pad="7"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="7"/>
<contactref element="R3" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="4"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="3"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="3"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="6"/>
<contactref element="J2" pad="1"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="1"/>
<contactref element="U$2" pad="6"/>
<contactref element="U$2" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
